# Chapter 1 View on RAM as a programmer

There is the memory in any PC, the fast random access memory called RAM.



Fig. -RAM device.

As a programmer you should think about the memory at the higher level than the physical device that you can see if you have dissembled system unit. So, all memory at the level of programming applications can be divided into three kinds.

First kind is a static memory. When you launch any application the operation system loads executable file of your application into the RAM. The operation system allocates memory for binary code and for variables and constants. This kind of memory lives until the application is closed. Operation system unloads all the application data from RAM after application was closed. So, “static” in this case means “to live while application works”. The size of static memory is not changed.

Second kind of memory is called “dynamic” or “heap”. When your application needs some additional memory it asks the operation system for that, and operation system allocates the memory if there is. When application no longer need early allocated memory it should return it back to operation system. So, this is why it is called “dynamic”.

Third kind of memory is called “stack”. It used by functions only. Each function has its own piece of stack memory.

Look at the fig.1-2 to view schematic image of memory used by application.

You always should understand in which piece of memory your data is located. For remember this kinds of memory you can use abbreviation “SSD” (Stack, Static, Dynamic). Ok, move on.




Fig. -Application memory.